show running-config

!Current Configuration:
!
!Parameter string escape handling \, 1
!Characters to be preceded with escape char (\): \, !, ", ', ?

!System Description "Hirschmann Railswitch"
! Version: L2P-09.0.14 Build: 2018-03-14 20:32
! Configuration state: OK
! Configuration signature: 53 5f 62 07
!clibanner

!Pre-login banner


vlan database
vlan  51 
vlan name 51 "Admin_Switch" 
vlan  52 
vlan name 52 "Reserve0" 
vlan  53 
vlan name 53 "Billettique" 
vlan  54 
vlan name 54 "Videosurveillance" 
vlan  55 
vlan name 55 "Systeme_information_voyageurs" 
vlan  56 
vlan name 56 "Sonorisation" 
vlan  57 
vlan name 57 "Signalisation_Alarmes_techniques" 
vlan  58 
vlan name 58 "Reseau_sans_fil" 
vlan  59 
vlan name 59 "RESERVE" 
vlan  60 
vlan name 60 "telephonie Interphonie" 
vlan  61 
vlan name 61 "Systeme_aide_exploitation" 
vlan  62 
vlan name 62 "Controle_acces" 
vlan  63 
vlan name 63 "Bureautique" 
vlan  64 
vlan name 64 "Reserve2" 
vlan  65 
vlan name 65 "Reserve3" 
vlan  66 
vlan name 66 "Reserve4" 
vlan  100 
vlan name 100 "Vlan_transfert" 
exit 

network protocol none
network parms 172.17.16.6 255.255.128.0 172.17.127.254
network mgmt_vlan 51 
network priority dot1p-vlan 7 
!RMA operation
!RMA entry
ip ssh protocol 1  


configure 

snmp-server sysname "MAV-PDP-L1 "
snmp-server location "Armoire AGI en station"
snmp-server contact "Antenne MAV Metro Ligne 1"
!


interface  1/1 
name "Vers RCM-PDP-L1"
no auto-negotiate
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
dhcp-server operation disable
set igmp forward-all
set igmp automatic-mode

spanning-tree guard loop

vlan pvid 51 
vlan participation auto 1 
vlan participation include 51 
vlan tagging 51 
vlan participation include 54 
vlan tagging 54 
vlan participation include 56 
vlan tagging 56 
vlan participation include 57 
vlan tagging 57 
port-monitor action port-disable
exit


interface  1/2 
name "MAINTENANCE"
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
dhcp-server operation disable
no set igmp

spanning-tree edgeport

vlan pvid 51 
vlan participation auto 1 
vlan participation include 51 
vlan tagging 51 
port-monitor action port-disable
exit


interface  1/3 
name "MAV - Sono"
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
set igmp static-query-port

spanning-tree edgeport

vlan pvid 56 
vlan participation auto 1 
vlan participation include 56 
port-monitor action port-disable
exit


interface  1/4 
name "MAV - Sono"
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
set igmp static-query-port

spanning-tree edgeport

vlan pvid 56 
vlan participation auto 1 
vlan participation include 56 
port-monitor action port-disable
exit


interface  1/5 
name "MAV - Sono"
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
set igmp static-query-port

spanning-tree edgeport

vlan pvid 56 
vlan participation auto 1 
vlan participation include 56 
port-monitor action port-disable
exit


interface  1/6 
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
shutdown
no set igmp

spanning-tree edgeport

vlan pvid 56 
vlan participation auto 1 
vlan participation include 56 
port-monitor action port-disable
exit


interface  1/7 
name "MAV - Sono (reserve)"
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
set igmp static-query-port

spanning-tree edgeport

vlan pvid 56 
vlan participation auto 1 
vlan participation include 56 
port-monitor action port-disable
exit


interface  1/8 
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
shutdown
no set igmp

spanning-tree edgeport

vlan pvid 56 
vlan participation auto 1 
vlan participation include 56 
port-monitor action port-disable
exit

snmptrap public 172.17.101.99
snmptrap public 172.17.101.100
snmptrap 0 172.17.16.90

!Address Conflict Detection

!Bridge Address Learning

!Bridge Fast Link Detection

!Maximum size of frame (packet size)

!Bridge Address Relearn Detection

!Bridge Address Relearn Threshold

!Bridge Duplex Mismatch Detection

!Bridge Hash Optimizing

!Service Mode

!VLAN Learning


!Hirschmann DHCP Relay

!Hirschmann Device Status
device-status monitor aca-removal error
device-status monitor power-supply-2 ignore
device-status monitor temperature error
device-status trap enable


!DHCP Server
!DHCP Server pools


!DIP Switch Admin State
dip-switch operation disable


!Ethernet/IP


!Mac Notification Global State



!Power over Ethernet (IEEE 802.3af)
!Selftest

!Skip ACA on boot


!Hirschmann HIPER Ring

!LLDP (IEEE802.1AB Link Layer Discovery Protocol)


!Media Redundancy Protocol (IEC 62439-2/Ed1.0, MRP)
!No MRP domains exist.

!Advanced Ring Configuration and Diagnostics


!No entries in alarm table

!MAC/IP Based Port Security
port-sec mode ip-based


!Port Monitor


!Auto Disable


!ProfinetIO


!Hirschmann Precision Time Protocol (PTP, IEEE 1588)

!Hirschmann Ring Coupling
!Note: master/slave (also for single) part of configuration determined by
!      management

!Hirschmann Signal Contacts
signal-contact 1 state closed
signal-contact 1 trap enable


!Hirschmann SNMP Access Control
snmp-access version v3-encryption readwrite enable


!SNMP Sync
no snmp sync v3-to-community


!SNTP
sntp operation on
sntp operation server off


!Hirschmann Broadcast Limiter


!Hirschmann Temperature Limit Settings
temperature upper-limit 50

users passwd admin :v1:81449548fb49a99bbfe64c92dbc8791f2e7975897283a71a3ad9f2452de95815:
users snmpv3 authentication admin md5
users snmpv3 encryption admin des :v1:81449548fb49a99bbfe64c92dbc8791f2e7975897283a71a3ad9f2452de95815:
users passwd user :v1:81439e52f35eccebbaf6498dd9cc690d307960987384bb0130dfe65324f0490c:
users snmpv3 authentication user md5
users snmpv3 encryption user des :v1:81439e52f35eccebbaf6498dd9cc690d307960987384bb0130dfe65324f0490c:


lineconfig
exit 


!IGMP Snooping
exit 


(Hirschmann Railswitch) #