show running-config all

!Current Configuration:
!
!Parameter string escape handling \, 1
!Characters to be preceded with escape char (\): \, !, ", ', ?

!System Description "Hirschmann Railswitch"
! Version: L2P-09.0.14 Build: 2018-03-14 20:32
! Configuration state: OK
! Configuration signature: 53 5f 62 07
!clibanner

no set clibanner operation 
!Pre-login banner

no set pre-login-banner operation 
set prompt "Hirschmann Railswitch"
no set gvrp adminmode
telnetcon timeout 5 
telnetcon maxsessions 5 

vlan database
vlan0-transparent-mode disable
vlan  1 
vlan  51 
vlan name 51 "Admin_Switch" 
vlan  52 
vlan name 52 "Reserve0" 
vlan  53 
vlan name 53 "Billettique" 
vlan  54 
vlan name 54 "Videosurveillance" 
vlan  55 
vlan name 55 "Systeme_information_voyageurs" 
vlan  56 
vlan name 56 "Sonorisation" 
vlan  57 
vlan name 57 "Signalisation_Alarmes_techniques" 
vlan  58 
vlan name 58 "Reseau_sans_fil" 
vlan  59 
vlan name 59 "RESERVE" 
vlan  60 
vlan name 60 "telephonie Interphonie" 
vlan  61 
vlan name 61 "Systeme_aide_exploitation" 
vlan  62 
vlan name 62 "Controle_acces" 
vlan  63 
vlan name 63 "Bureautique" 
vlan  64 
vlan name 64 "Reserve2" 
vlan  65 
vlan name 65 "Reserve3" 
vlan  66 
vlan name 66 "Reserve4" 
vlan  100 
vlan name 100 "Vlan_transfert" 
exit 

network protocol none
network protocol hidiscovery read-write
network parms 172.17.16.6 255.255.128.0 172.17.127.254
network mgmt_vlan 51 
network priority dot1p-vlan 7 
network priority ip-dscp 0 
!RMA operation
network mgmt-access operation disable
!RMA entry
network mgmt-access modify 1 ip 0.0.0.0
network mgmt-access modify 1 mask 0.0.0.0
network mgmt-access modify 1 http enable
network mgmt-access modify 1 https enable
network mgmt-access modify 1 snmp enable
network mgmt-access modify 1 telnet enable
network mgmt-access modify 1 ssh enable
network mgmt-access status 1 enable
ip http server
no ip https server
ip https port 443 
no ip ssh
ip ssh protocol 1  
sshcon maxsessions 5
sshcon timeout 5


configure 

snmp-server sysname "MAV-PDP-L1 "
snmp-server location "Armoire AGI en station"
snmp-server contact "Antenne MAV Metro Ligne 1"
!

no set gmrp adminmode
set gmrp forward-unknown flood
classofservice dot1p-mapping 0 1
classofservice dot1p-mapping 1 0
classofservice dot1p-mapping 2 0
classofservice dot1p-mapping 3 1
classofservice dot1p-mapping 4 2
classofservice dot1p-mapping 5 2
classofservice dot1p-mapping 6 3
classofservice dot1p-mapping 7 3
classofservice ip-dscp-mapping 0 1
classofservice ip-dscp-mapping 1 1
classofservice ip-dscp-mapping 2 1
classofservice ip-dscp-mapping 3 1
classofservice ip-dscp-mapping 4 1
classofservice ip-dscp-mapping 5 1
classofservice ip-dscp-mapping 6 1
classofservice ip-dscp-mapping 7 1
classofservice ip-dscp-mapping 8 0
classofservice ip-dscp-mapping 9 0
classofservice ip-dscp-mapping 10 0
classofservice ip-dscp-mapping 11 0
classofservice ip-dscp-mapping 12 0
classofservice ip-dscp-mapping 13 0
classofservice ip-dscp-mapping 14 0
classofservice ip-dscp-mapping 15 0
classofservice ip-dscp-mapping 16 0
classofservice ip-dscp-mapping 17 0
classofservice ip-dscp-mapping 18 0
classofservice ip-dscp-mapping 19 0
classofservice ip-dscp-mapping 20 0
classofservice ip-dscp-mapping 21 0
classofservice ip-dscp-mapping 22 0
classofservice ip-dscp-mapping 23 0
classofservice ip-dscp-mapping 24 1
classofservice ip-dscp-mapping 25 1
classofservice ip-dscp-mapping 26 1
classofservice ip-dscp-mapping 27 1
classofservice ip-dscp-mapping 28 1
classofservice ip-dscp-mapping 29 1
classofservice ip-dscp-mapping 30 1
classofservice ip-dscp-mapping 31 1
classofservice ip-dscp-mapping 32 2
classofservice ip-dscp-mapping 33 2
classofservice ip-dscp-mapping 34 2
classofservice ip-dscp-mapping 35 2
classofservice ip-dscp-mapping 36 2
classofservice ip-dscp-mapping 37 2
classofservice ip-dscp-mapping 38 2
classofservice ip-dscp-mapping 39 2
classofservice ip-dscp-mapping 40 2
classofservice ip-dscp-mapping 41 2
classofservice ip-dscp-mapping 42 2
classofservice ip-dscp-mapping 43 2
classofservice ip-dscp-mapping 44 2
classofservice ip-dscp-mapping 45 2
classofservice ip-dscp-mapping 46 2
classofservice ip-dscp-mapping 47 2
classofservice ip-dscp-mapping 48 3
classofservice ip-dscp-mapping 49 3
classofservice ip-dscp-mapping 50 3
classofservice ip-dscp-mapping 51 3
classofservice ip-dscp-mapping 52 3
classofservice ip-dscp-mapping 53 3
classofservice ip-dscp-mapping 54 3
classofservice ip-dscp-mapping 55 3
classofservice ip-dscp-mapping 56 3
classofservice ip-dscp-mapping 57 3
classofservice ip-dscp-mapping 58 3
classofservice ip-dscp-mapping 59 3
classofservice ip-dscp-mapping 60 3
classofservice ip-dscp-mapping 61 3
classofservice ip-dscp-mapping 62 3
classofservice ip-dscp-mapping 63 3

interface  1/1 
name "Vers RCM-PDP-L1"
no auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation disable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
set igmp
set igmp forward-all
no set igmp static-query-port
set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
spanning-tree guard loop
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 51 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation include 51 
vlan tagging 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation include 54 
vlan tagging 54 
vlan participation auto 55 
vlan participation include 56 
vlan tagging 56 
vlan participation include 57 
vlan tagging 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
no mode dvlan-tunnel 
exit


interface  1/2 
name "MAINTENANCE"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation disable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
no set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 51 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation include 51 
vlan tagging 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation auto 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit


interface  1/3 
name "MAV - Sono"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation enable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
set igmp
no set igmp forward-all
set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 56 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation include 56 
no vlan tagging 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit


interface  1/4 
name "MAV - Sono"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation enable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
set igmp
no set igmp forward-all
set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 56 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation include 56 
no vlan tagging 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit


interface  1/5 
name "MAV - Sono"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation enable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
set igmp
no set igmp forward-all
set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 56 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation include 56 
no vlan tagging 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit


interface  1/6 
no name
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation enable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
no set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 56 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation include 56 
no vlan tagging 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit


interface  1/7 
name "MAV - Sono (reserve)"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation enable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
set igmp
no set igmp forward-all
set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 56 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation include 56 
no vlan tagging 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit


interface  1/8 
no name
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias on
lldp tlv pnio-mrp off
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
lldp med
no lldp med confignotification
lldp med transmit-tlv capabilities
lldp med transmit-tlv network-policy
dhcp-server operation enable
no voice vlan 
voice vlan auth enable
dot1x port-control force-authorized 
no dot1x re-authentication 
dot1x timeout quiet-period 60
dot1x timeout reauth-period 3600
dot1x timeout supp-timeout 30
dot1x timeout tx-period 30
dot1x max-users 16
dot1x guest-vlan 0
dot1x timeout guest-vlan-period 90
dot1x timeout server-timeout 30
dot1x max-req 2
dot1x unauthenticated-vlan 0
dot1x mac-auth-bypass
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
snmp trap link-status
set garp timer join 20
set garp timer leave 60
set garp timer leaveall 1000
no set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
mac notification mode all
no mac notification operation

set gmrp interfacemode
no set gmrp forward-all-groups
set gvrp interfacemode
no spanning-tree guard
no spanning-tree tcnguard
spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 56 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation auto 52 
vlan participation auto 53 
vlan participation auto 54 
vlan participation auto 55 
vlan participation include 56 
no vlan tagging 56 
vlan participation auto 57 
vlan participation auto 58 
vlan participation auto 59 
vlan participation auto 60 
vlan participation auto 61 
vlan participation auto 62 
vlan participation auto 63 
vlan participation auto 64 
vlan participation auto 65 
vlan participation auto 66 
vlan participation auto 100 
vlan priority 0 
port-monitor disable
port-monitor condition link-flap disable
port-monitor condition crc-fragment disable
port-monitor condition overload-detection disable
port-monitor condition speed-duplex-monitor disable
port-monitor condition speed-duplex-monitor speed hdx-10 fdx-10 hdx-100 fdx-100 hdx-1000 fdx-1000
port-monitor action port-disable
port-monitor condition overload-detection traffic-type bc
port-monitor condition overload-detection threshold-type pps
port-monitor condition overload-detection upper-threshold 0
port-monitor condition overload-detection lower-threshold 0
auto-disable timer 0
profinetio dcp-mode both
profinetio fast-start-up disable
no mode dvlan-tunnel 
exit

no link-aggregation staticcapability

logging buffered
logging buffered wrap
no logging console
no logging syslog
no logging syslog port
logging snmp-requests get operation disable
logging snmp-requests get severity 5
logging snmp-requests set operation disabled
logging snmp-requests set severity 5
snmptrap public 172.17.101.99
snmptrap public 172.17.101.100
snmptrap 0 172.17.16.90

!Address Conflict Detection
address-conflict detection-mode disable
address-conflict ongoing-detection enable

!Bridge Address Learning
bridge address-learning enable

!Bridge Fast Link Detection
bridge fast-link-detection enable

!Maximum size of frame (packet size)
bridge framesize 1522

!Bridge Address Relearn Detection
bridge address-relearn-detect operation disable

!Bridge Address Relearn Threshold
bridge address-relearn-detect threshold 1

!Bridge Duplex Mismatch Detection
bridge duplex-mismatch-detect enable

!Bridge Hash Optimizing
bridge hash-optimizing mode 2

!Service Mode
bridge service-mode disable

!VLAN Learning
bridge vlan-learning independent


!Hirschmann DHCP Relay
dhcp-relay server-address 1 0.0.0.0 all     
dhcp-relay server-address 2 0.0.0.0 all     
dhcp-relay server-address 3 0.0.0.0 all     
dhcp-relay server-address 4 0.0.0.0 all     
dhcp-relay server-address 5 0.0.0.0 all     
dhcp-relay server-address 6 0.0.0.0 all     
dhcp-relay server-address 7 0.0.0.0 all     
dhcp-relay server-address 8 0.0.0.0 all     
dhcp-relay server-address 9 0.0.0.0 all     
dhcp-relay server-address 10 0.0.0.0 all     
dhcp-relay server-address 11 0.0.0.0 all     
dhcp-relay server-address 12 0.0.0.0 all     
dhcp-relay server-address 13 0.0.0.0 all     
dhcp-relay server-address 14 0.0.0.0 all     
dhcp-relay server-address 15 0.0.0.0 all     
dhcp-relay server-address 16 0.0.0.0 all     
dhcp-relay opt82 operation disable
dhcp-relay opt82 remote-id-type mac
no dhcp-relay opt82 man-id

!Hirschmann Device Status
device-status monitor aca-not-in-sync ignore
device-status monitor aca-removal error
device-status monitor connection-error ignore
device-status monitor hiper-ring ignore
device-status monitor power-supply-1 error
device-status monitor power-supply-2 ignore
device-status monitor ring-coupling ignore
device-status monitor temperature error
device-status trap enable


!DHCP Server
dhcp-server operation disable
dhcp-server addr-probe enable
!DHCP Server pools


!DIP Switch Admin State
dip-switch operation disable


!Ethernet/IP
ethernet-ip admin-state disable


!Mac Notification Global State
no mac notification operation
mac notification interval 1 


no mac-address-conflict operation

!Power over Ethernet (IEEE 802.3af)
inlinepower admin-mode enable
inlinepower trap enable
inlinepower threshold 90
!Selftest
selftest ramtest enable
selftest reboot-on-error enable
selftest reboot-on-hdxerror enable
selftest sysmon enable

!Skip ACA on boot
boot skip-aca-on-boot disable


!Hirschmann HIPER Ring
!Note: hiper-ring mode not configured
!Note: hiper-ring port primary not configured
!Note: hiper-ring port secondary not configured
hiper-ring recovery-delay 500ms

!LLDP (IEEE802.1AB Link Layer Discovery Protocol)
lldp
lldp config chassis notification-interval 5
lldp config chassis re-init-delay 2
lldp config chassis tx-delay 2
lldp config chassis tx-hold-mult 4
lldp config chassis tx-interval 30
lldp med faststartrepeatcount 3


!Media Redundancy Protocol (IEC 62439-2/Ed1.0, MRP)
!No MRP domains exist.

!Advanced Ring Configuration and Diagnostics
arc client enable
arc manager disable
arc protocol mrp


!No entries in alarm table

!MAC/IP Based Port Security
port-sec mode ip-based


!Port Monitor
port-monitor disable
port-monitor condition link-flap interval 10
port-monitor condition link-flap count 5
port-monitor condition crc-fragment interval 10
port-monitor condition crc-fragment count 1000
port-monitor condition overload-detection polling-interval 1


!Auto Disable
no auto-disable reason link-flap
no auto-disable reason crc-error
no auto-disable reason overload-detection
no auto-disable reason port-security
no auto-disable reason speed-duplex


!ProfinetIO
profinetio admin-state disable


!Hirschmann Precision Time Protocol (PTP, IEEE 1588)
ptp operation disable
ptp clock-mode v1-simple-mode

!Hirschmann Ring Coupling
!Note: master/slave (also for single) part of configuration determined by
!      management
ring-coupling port local 1/4
ring-coupling config dual-master-inband
ring-coupling redundancy-mode extended
ring-coupling net-coupling ring-only
ring-coupling operation off

!Hirschmann Signal Contacts
signal-contact 1 mode device-status
signal-contact 1 monitor aca-not-in-sync disable
signal-contact 1 monitor aca-removal disable
signal-contact 1 monitor connection-error disable
signal-contact 1 monitor hiper-ring disable
signal-contact 1 monitor power-supply-1 enable
signal-contact 1 monitor power-supply-2 enable
signal-contact 1 monitor ring-coupling disable
signal-contact 1 monitor temperature disable
signal-contact 1 state closed
signal-contact 1 trap enable


!Hirschmann SNMP Access Control
snmp-access global enable
snmp-access version v1 enable
snmp-access version v2 enable
snmp-access radius-authenticate disable
snmp-access version v3-encryption readonly disable
snmp-access version v3-encryption readwrite enable


!SNMP Sync
no snmp sync v3-to-community


!SNTP
sntp anycast address 0.0.0.0
sntp anycast transmit-interval 120
sntp anycast vlan 1
sntp client accept-broadcast on
sntp client disable-after-sync off
sntp client request-interval 30
sntp client offset 60
sntp client server primary 0.0.0.0
sntp client server secondary 0.0.0.0
sntp client threshold 0
sntp operation on
sntp operation server off
sntp operation client on
sntp server disable-if-local off


!Hirschmann Broadcast Limiter
no storm-control broadcast
storm-control egress-limiting disable
storm-control ingress-limiting disable


!Hirschmann Temperature Limit Settings
temperature lower-limit 0
temperature upper-limit 50

users passwd admin :v1:81449548fb49a99bbfe64c92dbc8791f2e7975897283a71a3ad9f2452de95815:
users access admin readwrite
users snmpv3 authentication admin md5
users snmpv3 encryption admin des :v1:81449548fb49a99bbfe64c92dbc8791f2e7975897283a71a3ad9f2452de95815:
users passwd user :v1:81439e52f35eccebbaf6498dd9cc690d307960987384bb0130dfe65324f0490c:
users access user readonly
users snmpv3 authentication user md5
users snmpv3 encryption user des :v1:81439e52f35eccebbaf6498dd9cc690d307960987384bb0130dfe65324f0490c:
users login admin defaultList
users login user defaultList
users defaultlogin radiuslist
no dot1x system-auth-control 
no authorization network radius 
no dot1x dynamic-vlan enable 
no dot1x safe-vlan 
dot1x login admin  radiuslist
dot1x login user  radiuslist
dot1x defaultlogin radiuslist
no voice vlan
no radius accounting mode
radius server retransmit 4 
radius server timeout 5

no monitor session 1 mode

lineconfig
serial timeout 5
transport input telnet
transport output telnet
session-timeout 5 
session-limit 5 
exit 

no storm-control flowcontrol
spanning-tree
spanning-tree configuration name "Default-6C-3A-22"
spanning-tree configuration revision 0
no spanning-tree bpduguard
spanning-tree forward-time 15 
spanning-tree max-age 20 
spanning-tree max-hops 20 
spanning-tree hello-time 2 
spanning-tree hold-count 10 
spanning-tree forceversion 802.1w 
no spanning-tree stp-mrp-mode
spanning-tree mst priority 0 32768
snmp-server community ipaddr 0.0.0.0 "public"
snmp-server community ipmask 0.0.0.0 "public"
snmp-server community ro "public"
snmp-server community ipaddr 0.0.0.0 "private"
snmp-server community ipmask 0.0.0.0 "private"
snmp-server community rw "private"
bridge aging-time 30 
snmp-server enable traps
snmp-server enable traps chassis
snmp-server enable traps l2redundancy
snmp-server enable traps linkmode
snmp-server enable traps multiusers
snmp-server enable traps port-sec
snmp-server enable traps stpmode

!IGMP Snooping
no set igmp
set igmp forward-unknown flood
set igmp querier status disable
set igmp querier protocol-version 2
! -- Order-sensitive commands, ID 1, begin
set igmp maxresponse 10
set igmp querier tx-interval 125
set igmp groupmembership-interval 260 
! -- Order-sensitive commands, ID 1, end
! -- Order-sensitive commands, ID 2, begin
set igmp lookup-resp-time-unknown 10
set igmp lookup-interval-unknown 125
set igmp aging-time-unknown 260
! -- Order-sensitive commands, ID 2, end
set igmp query-ports-to-filter disable
dvlan-tunnel ethertype 802.1Q 
exit 


(Hirschmann Railswitch) #