show running-config all

!Current Configuration:
!
!Parameter string escape handling \, 1
!Characters to be preceded with escape char (\): \, !, ", ', ?

!System Description "Hirschmann Railswitch"
! Version: L2E-09.0.14 Build: 2018-03-15 00:30
! Configuration state: OK
! Configuration signature: cb 35 ea c6
!clibanner

no set clibanner operation 
set prompt "Hirschmann Railswitch"
telnetcon timeout 5 
telnetcon maxsessions 2 

vlan database
vlan0-transparent-mode disable
vlan  1 
vlan  51 
vlan name 51 "Admin_Switch" 
vlan  53 
vlan name 53 "Billettique" 
vlan  250 
vlan name 250 "Anneau_MRP" 
exit 

network protocol none
network protocol hidiscovery read-write
network parms 172.17.28.47 255.255.128.0 172.17.127.254
network mgmt_vlan 51 
network priority dot1p-vlan 0 
network priority ip-dscp 0 
ip http server

configure 

snmp-server sysname "SWI.0.PHA.SDB.02"
snmp-server location "Salle_des_billets_Phalempins "
snmp-server contact "Antenne CAS Metro Ligne 2"
!

classofservice dot1p-mapping 0 1
classofservice dot1p-mapping 1 0
classofservice dot1p-mapping 2 0
classofservice dot1p-mapping 3 1
classofservice dot1p-mapping 4 2
classofservice dot1p-mapping 5 2
classofservice dot1p-mapping 6 3
classofservice dot1p-mapping 7 3
classofservice ip-dscp-mapping 0 1
classofservice ip-dscp-mapping 1 1
classofservice ip-dscp-mapping 2 1
classofservice ip-dscp-mapping 3 1
classofservice ip-dscp-mapping 4 1
classofservice ip-dscp-mapping 5 1
classofservice ip-dscp-mapping 6 1
classofservice ip-dscp-mapping 7 1
classofservice ip-dscp-mapping 8 0
classofservice ip-dscp-mapping 9 0
classofservice ip-dscp-mapping 10 0
classofservice ip-dscp-mapping 11 0
classofservice ip-dscp-mapping 12 0
classofservice ip-dscp-mapping 13 0
classofservice ip-dscp-mapping 14 0
classofservice ip-dscp-mapping 15 0
classofservice ip-dscp-mapping 16 0
classofservice ip-dscp-mapping 17 0
classofservice ip-dscp-mapping 18 0
classofservice ip-dscp-mapping 19 0
classofservice ip-dscp-mapping 20 0
classofservice ip-dscp-mapping 21 0
classofservice ip-dscp-mapping 22 0
classofservice ip-dscp-mapping 23 0
classofservice ip-dscp-mapping 24 1
classofservice ip-dscp-mapping 25 1
classofservice ip-dscp-mapping 26 1
classofservice ip-dscp-mapping 27 1
classofservice ip-dscp-mapping 28 1
classofservice ip-dscp-mapping 29 1
classofservice ip-dscp-mapping 30 1
classofservice ip-dscp-mapping 31 1
classofservice ip-dscp-mapping 32 2
classofservice ip-dscp-mapping 33 2
classofservice ip-dscp-mapping 34 2
classofservice ip-dscp-mapping 35 2
classofservice ip-dscp-mapping 36 2
classofservice ip-dscp-mapping 37 2
classofservice ip-dscp-mapping 38 2
classofservice ip-dscp-mapping 39 2
classofservice ip-dscp-mapping 40 2
classofservice ip-dscp-mapping 41 2
classofservice ip-dscp-mapping 42 2
classofservice ip-dscp-mapping 43 2
classofservice ip-dscp-mapping 44 2
classofservice ip-dscp-mapping 45 2
classofservice ip-dscp-mapping 46 2
classofservice ip-dscp-mapping 47 2
classofservice ip-dscp-mapping 48 3
classofservice ip-dscp-mapping 49 3
classofservice ip-dscp-mapping 50 3
classofservice ip-dscp-mapping 51 3
classofservice ip-dscp-mapping 52 3
classofservice ip-dscp-mapping 53 3
classofservice ip-dscp-mapping 54 3
classofservice ip-dscp-mapping 55 3
classofservice ip-dscp-mapping 56 3
classofservice ip-dscp-mapping 57 3
classofservice ip-dscp-mapping 58 3
classofservice ip-dscp-mapping 59 3
classofservice ip-dscp-mapping 60 3
classofservice ip-dscp-mapping 61 3
classofservice ip-dscp-mapping 62 3
classofservice ip-dscp-mapping 63 3

interface  1/1 
name "Boucle_CAS_Entree"
cable-crossing enable
no auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
speed 100 full-duplex
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation include 1 
vlan tagging 1 
vlan participation include 51 
vlan tagging 51 
vlan participation include 53 
vlan tagging 53 
vlan participation include 250 
vlan tagging 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/2 
name "Boucle_CAS_Sortie"
cable-crossing disable
no auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
speed 100 full-duplex
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation include 1 
vlan tagging 1 
vlan participation include 51 
vlan tagging 51 
vlan participation include 53 
vlan tagging 53 
vlan participation include 250 
vlan tagging 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/3 
name "Valideur_en_entree"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation include 53 
no vlan tagging 53 
vlan participation auto 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/4 
name "Valideur_en_sortie"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation include 53 
no vlan tagging 53 
vlan participation auto 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/5 
name "Carte_CPU_Portillon"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation include 53 
no vlan tagging 53 
vlan participation auto 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/6 
name "reserve"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation include 53 
no vlan tagging 53 
vlan participation auto 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/7 
name "Port_De_Service"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
no shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation include 53 
no vlan tagging 53 
vlan participation auto 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit


interface  1/8 
name "Reserve"
cable-crossing disable
auto-negotiate
dhcp-relay admin-state enable
dhcp-relay operation enable
dhcp-relay hirschmann-device disable
device-status connection-error ignore
lldp admin-state tx-and-rx
lldp fdb-mode auto-detect
lldp hm-mode rx-only
lldp max-neighbors 10
lldp notification off
lldp tlv link-aggregation on
lldp tlv mac-phy-config-state on
lldp tlv max-frame-size on
lldp tlv mgmt-addr on
lldp tlv pnio on
lldp tlv pnio-alias off
lldp tlv pnio-mrp on
lldp tlv port-desc on
lldp tlv port-vlan on
lldp tlv inlinepower on
lldp tlv protocol on
lldp tlv sys-cap on
lldp tlv sys-desc on
lldp tlv sys-name on
lldp tlv vlan-name on
lldp tlv gmrp on
lldp tlv igmp on
lldp tlv portsec on
lldp tlv ptp on
port-sec allowed-mac add 00:00:00:00:00:00/48
port-sec allowed-ip  add 0.0.0.0/32
port-sec action none
port-sec dynamic 0
shutdown
storm-control ingress-mode bc
storm-control ingress-limit 0
storm-control broadcast 0
storm-control egress-limit 0
storm-control flowcontrol
set igmp
no set igmp forward-all
no set igmp static-query-port
no set igmp automatic-mode
no spanning-tree guard
no spanning-tree tcnguard
no spanning-tree edgeport
spanning-tree auto-edgeport
spanning-tree hello-time 2 
spanning-tree port mode
spanning-tree mst 0 cost auto
spanning-tree mst 0 external-cost auto
spanning-tree mst 0 port-priority 128
utilization alarm-threshold lower 0
utilization alarm-threshold upper 0

vlan pvid 53 
vlan acceptframe all
no vlan ingressfilter
vlan participation auto 1 
vlan participation auto 51 
vlan participation include 53 
no vlan tagging 53 
vlan participation auto 250 
vlan priority 0 
profinetio dcp-mode both
profinetio fast-start-up disable
exit

logging buffered
logging buffered wrap
no logging console
no logging syslog
no logging syslog port
logging snmp-requests get operation disable
logging snmp-requests get severity 5
logging snmp-requests set operation disabled
logging snmp-requests set severity 5
snmptrap 0 172.17.28.200

!Address Conflict Detection
address-conflict detection-mode disable
address-conflict ongoing-detection enable

!Bridge Address Learning
bridge address-learning enable

!Bridge Fast Link Detection
bridge fast-link-detection enable

!Maximum size of frame (packet size)
bridge framesize 1522

!Bridge Address Relearn Detection
bridge address-relearn-detect operation disable

!Bridge Address Relearn Threshold
bridge address-relearn-detect threshold 1

!Bridge Duplex Mismatch Detection
bridge duplex-mismatch-detect enable

!Bridge Hash Optimizing
bridge hash-optimizing mode 2

!Service Mode
bridge service-mode disable

!VLAN Learning
bridge vlan-learning independent


!Hirschmann DHCP Relay
dhcp-relay server-address 1 0.0.0.0 all     
dhcp-relay server-address 2 0.0.0.0 all     
dhcp-relay server-address 3 0.0.0.0 all     
dhcp-relay server-address 4 0.0.0.0 all     
dhcp-relay server-address 5 0.0.0.0 all     
dhcp-relay server-address 6 0.0.0.0 all     
dhcp-relay server-address 7 0.0.0.0 all     
dhcp-relay server-address 8 0.0.0.0 all     
dhcp-relay server-address 9 0.0.0.0 all     
dhcp-relay server-address 10 0.0.0.0 all     
dhcp-relay server-address 11 0.0.0.0 all     
dhcp-relay server-address 12 0.0.0.0 all     
dhcp-relay server-address 13 0.0.0.0 all     
dhcp-relay server-address 14 0.0.0.0 all     
dhcp-relay server-address 15 0.0.0.0 all     
dhcp-relay server-address 16 0.0.0.0 all     
dhcp-relay opt82 operation disable
dhcp-relay opt82 remote-id-type mac
no dhcp-relay opt82 man-id

!Hirschmann Device Status
device-status monitor aca-not-in-sync ignore
device-status monitor aca-removal ignore
device-status monitor connection-error ignore
device-status monitor hiper-ring error
device-status monitor power-supply-1 error
device-status monitor power-supply-2 ignore
device-status monitor ring-coupling ignore
device-status monitor temperature ignore
device-status trap disable


!DIP Switch Admin State
dip-switch operation disable


!Ethernet/IP
ethernet-ip admin-state disable


no mac-address-conflict operation

!Power over Ethernet (IEEE 802.3af)
inlinepower admin-mode enable
inlinepower trap enable
inlinepower threshold 90
!Selftest
selftest ramtest enable
selftest reboot-on-error enable
selftest reboot-on-hdxerror enable
selftest sysmon enable

!Skip ACA on boot
boot skip-aca-on-boot disable


!Hirschmann HIPER Ring
!Note: hiper-ring mode not configured
!Note: hiper-ring port primary not configured
!Note: hiper-ring port secondary not configured
hiper-ring recovery-delay 500ms

!LLDP (IEEE802.1AB Link Layer Discovery Protocol)
lldp
lldp config chassis notification-interval 5
lldp config chassis re-init-delay 2
lldp config chassis tx-delay 2
lldp config chassis tx-hold-mult 4
lldp config chassis tx-interval 30

!Media Redundancy Protocol (IEC 62439-2/Ed1.0, MRP)
mrp new-domain default-domain
mrp current-domain advanced-mode enable
mrp current-domain manager-priority 32768
mrp current-domain mode client
mrp current-domain name ""
mrp current-domain recovery-delay 200ms
mrp current-domain port primary 1/1
mrp current-domain port secondary 1/2
mrp current-domain vlan 250
mrp current-domain operation enable

!MAC/IP Based Port Security
port-sec mode mac-based


!ProfinetIO
profinetio admin-state disable


!Hirschmann Precision Time Protocol (PTP, IEEE 1588)
ptp operation disable
ptp clock-mode v1-simple-mode

!Hirschmann Ring Coupling
!Note: master/slave (also for single) part of configuration determined by
!      management
ring-coupling port local 1/4
ring-coupling config dual-master-inband
ring-coupling redundancy-mode extended
ring-coupling net-coupling ring-only
ring-coupling operation off

!Hirschmann Signal Contacts
signal-contact 1 mode device-status
signal-contact 1 monitor aca-not-in-sync disable
signal-contact 1 monitor aca-removal disable
signal-contact 1 monitor connection-error disable
signal-contact 1 monitor hiper-ring disable
signal-contact 1 monitor power-supply-1 enable
signal-contact 1 monitor power-supply-2 enable
signal-contact 1 monitor ring-coupling disable
signal-contact 1 monitor temperature disable
signal-contact 1 state open
signal-contact 1 trap enable


!Hirschmann SNMP Access Control
snmp-access global enable
snmp-access version v1 enable
snmp-access version v2 enable


!SNMP Sync
no snmp sync v3-to-community


!SNTP
sntp anycast address 0.0.0.0
sntp anycast transmit-interval 120
sntp anycast vlan 1
sntp client accept-broadcast on
sntp client disable-after-sync off
sntp client request-interval 30
sntp client offset 60
sntp client server primary 0.0.0.0
sntp client server secondary 0.0.0.0
sntp client threshold 0
sntp operation on
sntp operation server off
sntp operation client on
sntp server disable-if-local off


!Hirschmann Broadcast Limiter
no storm-control broadcast
storm-control egress-limiting disable
storm-control ingress-limiting disable


!Hirschmann Temperature Limit Settings
temperature lower-limit 0
temperature upper-limit 70

users passwd admin :v1:975f845bfb48b8f4cff24c9cdfdd691b33766a906387a21c3cc9fa492df85f08:
users access admin readwrite
users snmpv3 authentication admin md5
users snmpv3 encryption admin none
users passwd user :v1:81439e52f35eccebbaf6498dd9cc690d307960987384bb0130dfe65324f0490c:
users access user readonly
users snmpv3 authentication user md5
users snmpv3 encryption user none
users login admin defaultList
users login user defaultList
users defaultlogin radiuslist
no monitor session 1 mode

lineconfig
serial timeout 5
transport input telnet
exit 

no storm-control flowcontrol
spanning-tree
spanning-tree configuration name "Default-65-98-DC"
spanning-tree configuration revision 0
spanning-tree bpduguard
spanning-tree forward-time 25 
spanning-tree max-age 39 
spanning-tree max-hops 20 
spanning-tree hello-time 2 
spanning-tree hold-count 10 
spanning-tree forceversion 802.1w 
spanning-tree stp-mrp-mode
spanning-tree mst priority 0 32768
snmp-server community ipaddr 0.0.0.0 "public"
snmp-server community ipmask 0.0.0.0 "public"
snmp-server community ro "public"
snmp-server community "fixeauto"
snmp-server community ipaddr 0.0.0.0 "fixeauto"
snmp-server community ipmask 0.0.0.0 "fixeauto"
snmp-server community rw "fixeauto"
bridge aging-time 30 
snmp-server enable traps
snmp-server enable traps chassis
snmp-server enable traps l2redundancy
snmp-server enable traps linkmode
snmp-server enable traps multiusers
snmp-server enable traps port-sec
snmp-server enable traps stpmode

!IGMP Snooping
set igmp
set igmp forward-unknown flood
set igmp querier status disable
set igmp querier protocol-version 2
! -- Order-sensitive commands, ID 1, begin
set igmp maxresponse 10
set igmp querier tx-interval 125
set igmp groupmembership-interval 260 
! -- Order-sensitive commands, ID 1, end
! -- Order-sensitive commands, ID 2, begin
set igmp lookup-resp-time-unknown 10
set igmp lookup-interval-unknown 125
set igmp aging-time-unknown 260
! -- Order-sensitive commands, ID 2, end
set igmp query-ports-to-filter disable
exit 


(Hirschmann Railswitch) #