show running-config

!Current Configuration:
!
!Parameter string escape handling \, 1
!Characters to be preceded with escape char (\): \, !, ", ', ?

!System Description "Hirschmann Railswitch"
! Version: L2E-09.0.14 Build: 2018-03-15 00:30
! Configuration state: OK
! Configuration signature: b2 af 05 13
!clibanner


vlan database
vlan  51 
vlan name 51 "Admin_Switch" 
vlan  53 
vlan name 53 "Billettique" 
vlan  250 
vlan name 250 "Anneau_MRP" 
exit 

network protocol none
network parms 172.17.3.42 255.255.128.0 172.17.127.254
network mgmt_vlan 51 

configure 

snmp-server sysname "SWI.0.TRI.SDB.04"
snmp-server location "Salle_des_billets_Triolo"
snmp-server contact "Antenne CAS Metro Ligne 1"
!


interface  1/1 
name "Boucle_CAS_Entree"
cable-crossing enable
no auto-negotiate

vlan pvid 53 
vlan tagging 1 
vlan participation include 51 
vlan tagging 51 
vlan participation include 53 
vlan tagging 53 
vlan participation include 250 
vlan tagging 250 
exit


interface  1/2 
name "Boucle_CAS_Sortie"
no auto-negotiate

vlan pvid 53 
vlan tagging 1 
vlan participation include 51 
vlan tagging 51 
vlan participation include 53 
vlan tagging 53 
vlan participation include 250 
vlan tagging 250 
exit


interface  1/3 
name "Valideur_en_entree"

vlan pvid 53 
vlan participation auto 1 
vlan participation include 53 
exit


interface  1/4 
name "Valideur_en_sortie"

vlan pvid 53 
vlan participation auto 1 
vlan participation include 53 
exit


interface  1/5 
name "Carte_CPU_Portillon"

vlan pvid 53 
vlan participation auto 1 
vlan participation include 53 
exit


interface  1/6 
name "Reserve"
shutdown

vlan pvid 53 
vlan participation auto 1 
vlan participation include 53 
exit


interface  1/7 
name "Port_De_Service"

vlan pvid 53 
vlan participation auto 1 
vlan participation include 53 
exit


interface  1/8 
name "Reserve"
shutdown

vlan pvid 53 
vlan participation auto 1 
vlan participation include 53 
exit

snmptrap 0 172.17.3.230

!Address Conflict Detection

!Bridge Address Learning

!Bridge Fast Link Detection

!Maximum size of frame (packet size)

!Bridge Address Relearn Detection

!Bridge Address Relearn Threshold

!Bridge Duplex Mismatch Detection

!Bridge Hash Optimizing

!Service Mode

!VLAN Learning


!Hirschmann DHCP Relay

!Hirschmann Device Status
device-status monitor hiper-ring error
device-status monitor power-supply-2 ignore


!DIP Switch Admin State
dip-switch operation disable


!Ethernet/IP



!Power over Ethernet (IEEE 802.3af)
!Selftest

!Skip ACA on boot


!Hirschmann HIPER Ring

!LLDP (IEEE802.1AB Link Layer Discovery Protocol)

!Media Redundancy Protocol (IEC 62439-2/Ed1.0, MRP)
mrp new-domain default-domain
mrp current-domain recovery-delay 200ms
mrp current-domain vlan 250
mrp current-domain operation enable

!MAC/IP Based Port Security


!ProfinetIO


!Hirschmann Precision Time Protocol (PTP, IEEE 1588)

!Hirschmann Ring Coupling
!Note: master/slave (also for single) part of configuration determined by
!      management

!Hirschmann Signal Contacts
signal-contact 1 trap enable


!Hirschmann SNMP Access Control


!SNMP Sync
no snmp sync v3-to-community


!SNTP
sntp operation on
sntp operation server off


!Hirschmann Broadcast Limiter


!Hirschmann Temperature Limit Settings

users passwd admin :v1:a3598a5be85cb8f4cfc64a92dfce7d1b33426c9e6394b61c3cfdfc472deb4b08:
users snmpv3 authentication admin md5
users passwd user :v1:81439e52f35eccebbaf6498dd9cc690d307960987384bb0130dfe65324f0490c:
users snmpv3 authentication user md5

lineconfig
exit 

spanning-tree configuration name "Default-65-98-DC"
spanning-tree bpduguard
spanning-tree forward-time 25 
spanning-tree max-age 39 
spanning-tree stp-mrp-mode
snmp-server community "fixeauto"

!IGMP Snooping
set igmp
exit 


(Hirschmann Railswitch) #